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	Fire Boss
	CL-215
	CL-415
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	Water Dropping Capacity
	799 Gal
	1,400 Gal
	1,600 Gal

	Foam Capabilities
	24 loads – Maximum
	20 Loads
	N/A (Current Contract)

	Gel Capabilities
	Load at Tanker Base
	N/A
	N/A

	Retardant Capabilities
	Load at Tanker Base
	N/A
	N/A

	Drop Height
	60-100 ft. above canopy
	100-200’ above Canopy
	100-200’ above Canopy

	Load Release
	Two Clamshell Doors – Computer Controlled Constant Flow – Salvo, String, or Split Drops – Coverage Level 1-6
	Two Doors –Computer Controlled, Single Operation, Sequence or Salvo
	Four Doors – Computer Controlled, Single Operation, Sequence or Salvo

	Type of Fuel
	Jet A
	100LL
	Jet A

	Fuel Burn/hour
	600 lbs/90 gal
	1000lbs/225 gal.
	1500lbs/350 gal.

	Min Runway Length
	3,000 gravel
	5,000 feet
	3,500 feet

	Water Scooping Distance (Touch down to lift off)
	2,000 feet
	2,000 feet
	2,000 feet

	Total Pickup distance to clear 50 foot obstacle
	5,668 feet
	5,280 feet
	4,400 feet

	Min. Scooping Water Depth
	4 ft.
	8 ft
	8 ft

	Headwind Limitations
	40 mph
	None
	None

	Crosswind
	20 knots
	22 knots
	22 knots

	Fuel Cycle
	3 hours
	4 hours
	4 hours

	Normal Cruise Speed
	140 knots
	150 knots
	170 knots

	Max. Cruise Speed
	155 knots
	164 knots
	187 knots



[bookmark: OLE_LINK1]Tanker Operations Safety
Tanker operations are potentially dangerous. The entire load can be released in seconds. From drop heights of 100-200 feet, this force can have a devastating effect on tree crowns and shallow rooted tree species. It is essential that all line personnel stay clear of the drop zones. 
Buffers around the drop zone must be maintained to provide a safe working environment for ground personnel.  
These minimum standards should be followed:  
· 200’ laterally for personnel & equipment 
· 300’ in front of or behind canopied equipment  
· 500’ in front of or behind unprotected personnel              
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